Shot Cam IP D-Link DCS-950/950G V1.00 MAH 8/2008

Tab "Capture Settings"
All parameters to fill in "Server setting Cam DCS-950" are the same as what you have in your pages administrator of the DCS-950, http://xxx.xxx.xxx.xxx/web/login. asp (xxx.xxx.xxx.xxx is the IP of your camera DCS-950).
(The password and the name in "Setup / Advanced / User" are those user, not an administrator).
The software generates images cyclically to the time interval in minutes programmed in "Timer".
Images captured are:
- "LastShot.jpg" in the installation directory "Shot Cam DCS-950". This is the last capture fundamental. It will be crushed by the capture follows.
- "Uploadwebcam.jpg" in the installation directory "Shot Cam DCS-950". This is the last catch with stamp date / time / name. It will be crushed by the capture follows.
- "Cam001.jpg" in the directory you specified in "Image Folder." This is the last catch with stamp date / time / name. It will be renamed "cam002.jpg" by following the capture ... then incremented each capture up "cam999.jpg."
Note
- For proper functioning of Shot Cam DCS-950, you must have MS Internet Explorer 6 or MS Internet Explorer 7 installed on your computer.
- Tested on Windows XP only.
- If you use the increment names of images, you need a directory only for those catches.
- It is recommended to work in 32-bit mode for display. (Best conversion JPG).

To transfer images on a website / ftp, you can use a program like "filezilla" (free) http://filezilla-project.org

Onglet "Capture Settings"

Tous les paramètres à renseigner dans "Server setting Cam DCS-950" sont les mêmes que ceux que vous avez dans vos pages d'administrateur de la DCS-950, http://xxx.xxx.xxx.xxx/web/login.asp (xxx.xxx.xxx.xxx est l'IP de votre camera DCS-950).
(Le mot de passe et le nom dans "Setup/Advanced/User" sont ceux d'utilisateur, et non d'administrateur).

Le logiciel génère les images cycliquement à l'intervalle de temps en minutes programmé dans "Timer".

Les images capturées sont :

- "lastShot.jpg" dans le répertoire d'installation de "Shot Cam DCS-950". C'est la dernière capture brute. Elle sera écrasée par la capture suivante.

- "uploadwebcam.jpg" dans le répertoire d'installation de "Shot Cam DCS-950". C'est la dernière capture avec les incrustations de date/heure/nom. Elle sera écrasée par la capture suivante.

- "cam001.jpg" dans le répertoire que vous avez spécifié dans "Image Folder". C'est la dernière capture avec les incrustations de date/heure/nom. Elle sera renommée en "cam002.jpg" par la capture suivante...puis incrémentée à chaque capture jusqu'à "cam999.jpg".

Remarques

- Pour un bon fonctionnement de Shot Cam DCS-950, vous devez avoir MS Internet explorer 6 ou MS Internet explorer 7 installé sur votre ordinateur.
- Testé que sur Windows XP.
- Si vous utilisez la fonction d'incrémentation des noms d'images, vous devez avoir un répertoire uniquement pour ces captures.
- Il est recommandé de travailler en mode 32 bits pour l'affichage. (Meilleure conversion JPG).

Pour le transfert des images sur un site Web/ftp, vous pourrez par exemple utiliser un logiciel comme "filezilla"(gratuit) http://www.filezilla.fr

Rev Mah 9/8/2008
http://marcodechaligny.free.fr/